
**Communication Test**



**Step1.** Connect the unit and the PC via RS-232 communication cable.



**Step2.** Once the unit has been properly installed and the batteries are connected well, simply press On/Off switch (located on the display panel) to turn on the unit. Make sure the LCD is lit normally.





**Step3.** Double click AxpertTools as refer to below.

**Step4.** Click “RS232” and then press “Search” button to get serial number on the “Product ID”.

And Press “Apply” button to setting serial number. If the setting is don after the tool mention you “Setting Successful”.

**Step10.** Please restart the unit (totally shutdown, remove AC input and PV input)